ADC Assignment

1. WAP to interface LDR to controller and take the reading.
2. Automate the LED using LDR values or Potentiometer values.