1. WAP to enable two interrupts, Turn ON LED through one interrupt and TURN OFF LED through another interrupt.
2. WAP to Blink LED in an ISR with the delay of 2000 ms.